**The Danish Defence Acquisition and Logistics Organization**

**Tender for Foam sleeping pads**

|  |  |  |
| --- | --- | --- |
| **Question submitted** | **Answer** | **Date of answering** |
| *Question no. 1:*  Please confirm that the thickness for the foam sleeping pads is 10-11 +/- 0,4 mm? | DALO has by mistake uploaded an old version of drawing 335498. The new version (Edition 5) with the new measurements is now available on udbud.dk.  The thickness of the Foam Sleeping pad shall be 11 mm +/- 0.5 mm.  Please note that the length, width and corner measurements are updated as well. | 20-11-2018 |
| *Question no. 2:*  Also, please confirm that there are no insulation requirements such as R-values for this foam sleeping pad? | DALO confirms that there are no requirements to insulation. Tenderers are welcome to state the R-value of the offered sleeping pad. |  |
| * *Question no.3*   Vil i have FMI logoet trykt eller ridset ind i liggeunderlaget?  Does DALO want the LOGO printed or scratched into the Foam sleeping pads | It is up to the tenderer how to mark the product with the three letters FMI and the production-year.  The marking can for example be done by print or permanent debossing.  The sample does not have to be marked. |  |
| * *Question no. 4*   I skriver Grommet sejlringe men hvilken str. Grommets  1 eller 2 osv. eller opgiv gerne  indvendig hul str. | There are no requirements to the size of the grommets.  The purpose of the grommet is to reinforce in order to avoid tearing of the foam. | 27.11.2018 |
| * *Question no. 5*   I må gerne beskrive pakningen lidt mere da Pads vil rage ca. 30cm ud på hver side af en Europalle 120x80cm. Strækfilm omkring? | Se ’Requirement Specification no. 11’.  Det er forventet, at underlagene sticker ca. 20 – 30 cm. Ud over hver ende af pallen.  Højde på pallen må max være 120 cm.  Se Terms and Conditions 6.1 |  |
| * *Question no. 6*   Noget ønske om antal pads pr. palle ? | Højde på pallen må max være 120 cm.  Se Terms and Conditions 6.1 |  |