**Requirement Specification for F-16 Upper Outboard Bulkhead Flange Fittings without coating finish**

1. **Requirements**

**1.1. Description of the requirement**

 **DALO require a total of 92 EA F-16 Upper Outboard Bulkhead Flange fittings for repair of RDAF F-16 Aircrafts. The fittings shall be produced according to latest version of Lockheed Martin’s drawing 16RB526, except for finishing specification S635, FPS-3001.**

|  |  |  |
| --- | --- | --- |
| **PN** | NSN | Antal |
| **16RB526-9** | 1560016239269 | 5 |
| **16RB526-10** | 1560016239277 | 6 |
| **16RB526-11** | 1560016239303 | 5 |
| **16RB526-12** | 1560016239970 | 6 |
| **16RB526-13** | 1560016239944 | 6 |
| **16RB526-14** | 1560016239950 | 6 |
| **16RB526-15** | 1560016239956 | 6 |
| **16RB526-16** | 1560016239966 | 6 |
| **16RB526-17** | 1560016240214 | 5 |
| **16RB526-18** | 1560016239939 | 6 |
| **16RB526-19** | 1560016239975 | 5 |
| **16RB526-20** | 1560016239977 | 6 |
| **16RB526-21** | 1560016239981 | 6 |
| **16RB526-22** | 1560016240204 | 6 |
| **16RB526-23** | 1560016239991 | 6 |
| **16RB526-24** | 1560016240036 | 6 |

**1.2. Description and definitions**

The requirement specification, cf. section 1.4, describes all the requirements for the acquisition and consists of six columns with the following information:

|  |  |
| --- | --- |
| "#" | ID number |
| "Requirement" | Requirement description |
| "Classification" | The classification of the requirement as further described in section 1.3 |
| "DALO remarks" | Further information regarding the requirement |
| "Requirement compliance" | The tenderer's indication of compliance (YES or NO) |
| "Tender description" | Requirements regarding the tenderer's compliance description  |

**1.3. Classification**

All requirements are mandatory requirements (SHALL) and shall be fulfilled by the tenderer. If just one of the mandatory requirements is not fulfilled, the tenderer's tender will not be taken into further consideration.

**1.4. Requirement and response sheet**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **#** | **Requirement** | **Classification** | **DALO remarks** | **To be filled out be the tenderer** |
| **Requirement compliance****(tick a box)** | **Tenderer's description** |
| **YES** | **NO** |
| **1** | The fittings SHALL be produced according to the latest version of Lockheed Martin’s drawing 16RB526, except the finish specification S635 IAW FPS-3001, Verify Heat Treatment per NDTS 1500, Penetrant inspection IAW NDTS 1101 and Parts Marking FPS-3008.  | SHALL |  |  |  |  |
| **2** | Each Fittings shall be able to complete “Verify Heat Treatment” IAW NDTS 1500 as approved item.  | SHALL | DALO will conduct the Verify Heat Treatment IAW NDTS 1500 and if the item does not meet requirement of this test, the item in question will not be accepted by DALO. |  |  |  |
| **3** | Each fitting (unit) SHALL have clear identification of dash Part Number. | SHALL | Can be non-damage and easy removable label/sticker on part or identification within the individual fitting packaging. |  |  |  |
| **4** | Producer of fittings SHALL be supplier of similar part for Lockheed Martin and/or US Air Force. Documentation of this cooperation must be submitted with the tender. | SHALL | For example a copy of a letter or email in which the manufacturer confirms to support the supplier in connection with sales to DALO. |  |  |  |