**Requirement Specification F-16 NLG Tires**

1. **Requirements**

**1.1. Description and definitions**

The requirement specification, cf. section 1.4, describes all the requirements for the acquisition and consists of six columns with the following information:

|  |  |
| --- | --- |
| "#" | ID number |
| "Requirement" | Requirement description |
| "Classification" | The classification of the requirement as further described in section 1.3 |
| "DALO remarks" | Further information regarding the requirement |
| "Requirement compliance" | The tenderer's indication of compliance (YES or NO) |
| "Tender description" | Requirements regarding the tenderer's compliance description |

**1.2. Classification**

All requirements are mandatory requirements (SHALL) and shall be fulfilled by the tenderer. If just one of the mandatory requirements is not fulfilled, the tenderer's tender will not be taken into further consideration.

**1.3. Requirement and response sheet**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **#** | **Requirement** | **Classification** | **DALO remarks** | **To be filled out be the tenderer** | | |
| **Requirement compliance** | | **Tenderer's description** |
| **YES** | **NO** |
| **1** | The Tires shall be authorized for use on F-16 A/B operating up to MTOW of 37.500 lbs. | SHALL |  |  |  |  |
| **2** | The Tires shall be P/N 461B-3563-TL or P/N 005-643-004. | SHALL |  |  |  |  |
| **3** | At least 30 ea Tires SHALL be delivered within 45 calendar days from signing of the Agreement. | SHALL |  |  |  |  |
| **4** | The remaining 70 ea. Tires SHALL be delivered within 90 calendar days from signing of the Agreement. | SHALL |  |  |  |  |
| **5** | The tires shall be newly manufactured. A production date older than January 2015 will not be accepted. | SHALL |  |  |  |  |