**Requirement Specification for**

**Cabled Remote Controls for DBAL-A3**

1. **Requirements**

**1.1. Description of the requirement**

DALO wants to acquire 600 pcs. of cabled remote controls as a re-supply for their existing stock of Laser Devices: Steiner eOPTICS DBAL-A3 tactical light-lasers.

The cabled remote controls are used to switch on and off the output of the devices’ light sources, including the external OV-2 white light.

DALO desires that all their DBAL-A3 sets’ stock is uniform and therefore it is envisaged that the parts offered for the re-supply are either original spare parts or parts that are identical in form, function and quality to the OEM parts, as listed in section 1.4.

**1.2. Description and definitions**

The requirement specification, cf. section 1.4, describes all the requirements for the acquisition and consists of six columns with the following information:

|  |  |
| --- | --- |
| "#" | ID number |
| "Requirement" | Requirement description |
| "Classification" | The classification of the requirement as further described in section 1.3 |
| "DALO remarks" | Further information regarding the requirement |
| "Requirement compliance" | The tenderer's indication of compliance (YES or NO) |
| "Tender description" | Requirements regarding the tenderer's compliance description  |

**1.3. Classification**

All requirements are mandatory requirements (SHALL) and shall be fulfilled by the tenderer. If just one of the mandatory requirements is not fulfilled, the tenderer's tender will not be taken into further consideration.

**1.4. Requirement and response sheet**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **#** | **Requirement** | **Classification** | **DALO remarks** | **To be filled out be the tenderer** |
| **Requirement compliance****(tick a box)** | **Tenderer's description** |
| **YES** | **NO** |
| **1** | The supplier shall be able to deliver the following items in the specified quantities:1. NSN: 6150015370495

Steiner eOPTICS P/N: FA05063-7CABLE,SWITCH 7IN ANGLE DBAL-A3Qty.: 3001. NSN: 6150016143203

Steiner eOPTICS P/N: FA06146-7-7CABLE,DUAL SWITCH 7IN DBAL-A3Qty.: 300 | SHALL |  |  |  |  |
| **2** | All of the parts shall be new and of no lesser quality than the OEM product referred to in Requirement ID No. 1.  | SHALL |  |  |  |  |
| **3** | Delivery time shall be no less than 120 days from submission of the purchase order. | SHALL |  |  |  |  |